### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.1 (WebPack) - M.53d | Target Family: | Spartan3A and Spartan3AN
OS Platform: | NT | Target Device: | xc3s400an
Project ID (random number) | 684acf2150724198a130877b888bb684.def4846622c0434d9c6d6a2cfeb80550.2 | Target Package: | fgg400
Registration ID | 176036481_0_0_631 | Target Speed: | -4
Date Generated | 2015-07-12T21:23:59 | Tool Flow | CommandLine

User Environment
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | Intel(R) Xeon(R) CPU W3520 @ 2.67GHz | CPU Speed | 2666 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
| MiscellaneousStatistics AGG_BONDED_IO=86 AGG_IO=86 AGG_SLICE=3435 NUM_4_INPUT_LUT=6091 NUM_BONDED_IBUF=49 NUM_BONDED_IOB=37 NUM_BUFGMUX=7 NUM_CARRY_SKIP=6 NUM_CYMUX=741 NUM_DCM=2 NUM_DP_RAM=128 NUM_IOB_FF=10 NUM_LUT_RT=196 NUM_MULT18X18SIO=2 NUM_RAMB16BWE=19 NUM_SHIFT=10 NUM_SLICEL=3331 NUM_SLICEM=104 NUM_SLICE_FF=1830 NUM_XOR=637 | NetStatistics NumNets_Active=6740 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BRAMADDR=226 NumNodesOfType_Active_BRAMDUMMY=296 NumNodesOfType_Active_CLKPIN=1267 NumNodesOfType_Active_CNTRLPIN=1891 NumNodesOfType_Active_DOUBLE=17100 NumNodesOfType_Active_DUMMY=19570 NumNodesOfType_Active_DUMMYBANK=237 NumNodesOfType_Active_DUMMYESC=24 NumNodesOfType_Active_GLOBAL=284 NumNodesOfType_Active_HFULLHEX=272 NumNodesOfType_Active_HLONG=56 NumNodesOfType_Active_HUNIHEX=1640 NumNodesOfType_Active_INPUT=21562 NumNodesOfType_Active_IOBOUTPUT=31 NumNodesOfType_Active_OMUX=6297 NumNodesOfType_Active_OUTPUT=6615 NumNodesOfType_Active_PREBXBY=4937 NumNodesOfType_Active_VFULLHEX=884 NumNodesOfType_Active_VLONG=155 NumNodesOfType_Active_VUNIHEX=1191 NumNodesOfType_Vcc_BRAMDUMMY=83 NumNodesOfType_Vcc_CNTRLPIN=7 NumNodesOfType_Vcc_DUMMY=10 NumNodesOfType_Vcc_INPUT=145 NumNodesOfType_Vcc_PREBXBY=48 NumNodesOfType_Vcc_VCCOUT=132 SiteStatistics IBUF-DIFFMLR=12 IBUF-DIFFMTB=12 IBUF-DIFFSLR=11 IBUF-DIFFSTB=12 IOB-DIFFMLR=3 IOB-DIFFMTB=15 IOB-DIFFSLR=4 IOB-DIFFSTB=15 SLICEL-SLICEM=1612 | SiteSummary BUFGMUX=7 BUFGMUX_GCLKMUX=7 BUFGMUX_GCLK_BUFFER=7 DCM=2 DCM_DCM=2 IBUF=49 IBUF_DELAY_ADJ_BBOX=49 IBUF_IFF1=8 IBUF_INBUF=49 IBUF_PAD=49 IOB=37 IOB_OFF1=2 IOB_OUTBUF=37 IOB_PAD=37 MULT18X18SIO=2 MULT18X18SIO_MULT18X18SIO=2 RAMB16BWE=19 RAMB16BWE_RAMB16BWE=19 SLICEL=3331 SLICEL_C1VDD=60 SLICEL_C2VDD=68 SLICEL_CYMUXF=390 SLICEL_CYMUXG=351 SLICEL_F=2961 SLICEL_F5MUX=507 SLICEL_F6MUX=18 SLICEL_FFX=974 SLICEL_FFY=814 SLICEL_G=2928 SLICEL_GNDF=189 SLICEL_GNDG=148 SLICEL_VDDG=6 SLICEL_XORF=327 SLICEL_XORG=310 SLICEM=104 SLICEM_F=98 SLICEM_F5MUX=32 SLICEM_F6MUX=32 SLICEM_FFX=2 SLICEM_FFY=40 SLICEM_G=104 SLICEM_WSGEN=72

Configuration Data
BUFGMUX S=[S_INV:7] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:7] S=[S_INV:7] [S:0] DCM PSCLK=[PSCLK_INV:0] [PSCLK:2] PSEN=[PSEN_INV:0] [PSEN:2] PSINCDEC=[PSINCDEC_INV:0] [PSINCDEC:2] RST=[RST:1] [RST_INV:1] DCM_DCM CLKDV_DIVIDE=[2:1] [16:1] CLKOUT_PHASE_SHIFT=[NONE:2] CLK_FEEDBACK=[1X:2] DESKEW_ADJUST=[9:2] DFS_FREQUENCY_MODE=[LOW:2] DLL_FREQUENCY_MODE=[LOW:2] DUTY_CYCLE_CORRECTION=[TRUE:2] FACTORY_JF1=[0XC0:2] FACTORY_JF2=[0X80:2] PSCLK=[PSCLK_INV:0] [PSCLK:2] PSEN=[PSEN_INV:0] [PSEN:2] PSINCDEC=[PSINCDEC_INV:0] [PSINCDEC:2] RST=[RST:1] [RST_INV:1] IBUF ICE=[ICE:8] [ICE_INV:0] ICLK1=[ICLK1_INV:0] [ICLK1:8] IBUF_DELAY_ADJ_BBOX DELAY_ADJ_ATTRBOX=[FIXED:49] IBUF_DELAY_VALUE=[DLY0:49] IFD_DELAY_VALUE=[DLY0:41] [DLY5:8] SEL_IN=[SEL_IN:49] [SEL_IN_INV:0] IBUF_IFF1 CE=[CE:8] [CE_INV:0] CK=[CK:8] [CK_INV:0] IFF1_INIT_ATTR=[INIT0:8] LATCH_OR_FF=[FF:8] IBUF_PAD IOATTRBOX=[LVTTL:49] IOB O1=[O1_INV:1] [O1:36] OTCLK1=[OTCLK1_INV:0] [OTCLK1:2] IOB_OFF1 CK=[CK:2] [CK_INV:0] D=[D:2] [D_INV:0] LATCH_OR_FF=[FF:2] OFF1_INIT_ATTR=[INIT0:2] IOB_OUTBUF IN=[IN_INV:1] [IN:36] SUSPEND=[3STATE:37] | IOB_PAD DRIVEATTRBOX=[12:37] IOATTRBOX=[LVTTL:37] SLEW=[SLOW:37] MULT18X18SIO CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] MULT18X18SIO_MULT18X18SIO AREG=[0:2] BREG=[0:2] B_INPUT=[DIRECT:2] CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] PREG=[0:2] PREG_CLKINVERSION=[0:2] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:19] CLKB=[CLKB_INV:0] [CLKB:2] ENA=[ENA_INV:0] [ENA:19] ENB=[ENB_INV:0] [ENB:2] SSRA=[SSRA_INV:0] [SSRA:19] SSRB=[SSRB_INV:0] [SSRB:2] WEA0=[WEA0:17] [WEA0_INV:2] WEA1=[WEA1:17] [WEA1_INV:2] WEA2=[WEA2:17] [WEA2_INV:2] WEA3=[WEA3_INV:2] [WEA3:17] WEB0=[WEB0:2] [WEB0_INV:17] WEB1=[WEB1:2] [WEB1_INV:17] WEB2=[WEB2_INV:17] [WEB2:2] WEB3=[WEB3:2] [WEB3_INV:17] RAMB16BWE_RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:19] CLKB=[CLKB_INV:0] [CLKB:2] DATA_WIDTH_A=[4:8] [9:10] [18:1] DATA_WIDTH_B=[0:17] [9:1] [18:1] ENA=[ENA_INV:0] [ENA:19] ENB=[ENB_INV:0] [ENB:2] SSRA=[SSRA_INV:0] [SSRA:19] SSRB=[SSRB_INV:0] [SSRB:2] WEA0=[WEA0:17] [WEA0_INV:2] WEA1=[WEA1:17] [WEA1_INV:2] WEA2=[WEA2:17] [WEA2_INV:2] WEA3=[WEA3_INV:2] [WEA3:17] WEB0=[WEB0:2] [WEB0_INV:17] WEB1=[WEB1:2] [WEB1_INV:17] WEB2=[WEB2_INV:17] [WEB2:2] WEB3=[WEB3:2] [WEB3_INV:17] WRITE_MODE_A=[WRITE_FIRST:19] WRITE_MODE_B=[WRITE_FIRST:19] | SLICEL BX=[BX_INV:22] [BX:774] BY=[BY:310] [BY_INV:18] CE=[CE:1091] [CE_INV:1] CIN=[CIN_INV:0] [CIN:341] CLK=[CLK:1148] [CLK_INV:12] SR=[SR:655] [SR_INV:22] SLICEL_CYMUXF 0=[0:390] [0_INV:0] 1=[1_INV:6] [1:384] SLICEL_CYMUXG 0=[0:345] [0_INV:0] SLICEL_F5MUX S0=[S0:507] [S0_INV:0] SLICEL_F6MUX S0=[S0:18] [S0_INV:0] SLICEL_FFX CE=[CE:928] [CE_INV:0] CK=[CK:974] [CK_INV:0] D=[D:958] [D_INV:16] FFX_INIT_ATTR=[INIT0:867] [INIT1:107] FFX_SR_ATTR=[SRLOW:871] [SRHIGH:103] LATCH_OR_FF=[FF:974] REV=[REV_INV:0] [REV:2] SR=[SR:539] [SR_INV:18] SYNC_ATTR=[ASYNC:911] [SYNC:63] SLICEL_FFY CE=[CE:759] [CE_INV:1] CK=[CK:802] [CK_INV:12] D=[D:796] [D_INV:18] FFY_INIT_ATTR=[INIT0:759] [INIT1:55] FFY_SR_ATTR=[SRLOW:761] [SRHIGH:53] LATCH_OR_FF=[FF:814] REV=[REV_INV:0] [REV:4] SR=[SR:424] [SR_INV:22] SYNC_ATTR=[ASYNC:730] [SYNC:84] SLICEL_XORF 1=[1_INV:6] [1:321] SLICEM BX=[BX_INV:0] [BX:34] BY=[BY:104] [BY_INV:0] CE=[CE:40] [CE_INV:0] CLK=[CLK:72] [CLK_INV:0] SR=[SR:72] [SR_INV:0] SLICEM_F DI=[DI:66] [DI_INV:0] F_ATTR=[DUAL_PORT:64] [SHIFT_REG:2] LUT_OR_MEM=[LUT:32] [RAM:66] | SLICEM_F5MUX S0=[S0:32] [S0_INV:0] SLICEM_F6MUX S0=[S0:32] [S0_INV:0] SLICEM_FFX CE=[CE:2] [CE_INV:0] CK=[CK:2] [CK_INV:0] D=[D:2] [D_INV:0] FFX_INIT_ATTR=[INIT0:2] FFX_SR_ATTR=[SRLOW:2] LATCH_OR_FF=[FF:2] SYNC_ATTR=[ASYNC:2] SLICEM_FFY CE=[CE:40] [CE_INV:0] CK=[CK:40] [CK_INV:0] D=[D:40] [D_INV:0] FFY_INIT_ATTR=[INIT0:40] FFY_SR_ATTR=[SRLOW:40] LATCH_OR_FF=[FF:40] SYNC_ATTR=[ASYNC:40] SLICEM_G DI=[DI:72] [DI_INV:0] G_ATTR=[DUAL_PORT:64] [SHIFT_REG:8] LUT_OR_MEM=[LUT:32] [RAM:72] SLICEM_WSGEN CK=[CK:72] [CK_INV:0] SYNC_ATTR=[ASYNC:40] WE=[WE_INV:0] [WE:72]

Pin Data
BUFGMUX I0=7 O=7 S=7 BUFGMUX_GCLKMUX I0=7 OUT=7 S=7 BUFGMUX_GCLK_BUFFER IN=7 OUT=7 DCM CLK0=2 CLKDV=1 CLKFB=2 CLKFX=1 CLKIN=2 LOCKED=1 PSCLK=2 PSEN=2 PSINCDEC=2 RST=2 STATUS2=1 DCM_DCM CLK0=2 CLKDV=1 CLKFB=2 CLKFX=1 CLKIN=2 LOCKED=1 PSCLK=2 PSEN=2 PSINCDEC=2 RST=2 STATUS2=1 IBUF I=41 ICE=8 ICLK1=8 IQ1=8 PAD=49 IBUF_DELAY_ADJ_BBOX IBUF_OUT=41 IFD_OUT=8 SEL_IN=49 IBUF_IFF1 CE=8 CK=8 D=8 Q=8 IBUF_INBUF IN=49 OUT=49 IBUF_PAD PAD=49 IOB O1=37 OTCLK1=2 PAD=37 IOB_OFF1 CK=2 D=2 Q=2 IOB_OUTBUF IN=37 OUT=37 IOB_PAD PAD=37 MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P16=2 P17=2 P18=2 P19=2 P20=2 P21=2 P22=2 P23=2 P24=2 P25=2 P26=2 P27=2 P28=2 P29=2 P30=2 P31=2 P32=2 P33=2 RSTA=2 RSTB=2 RSTP=2 | MULT18X18SIO_MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P16=2 P17=2 P18=2 P19=2 P20=2 P21=2 P22=2 P23=2 P24=2 P25=2 P26=2 P27=2 P28=2 P29=2 P30=2 P31=2 P32=2 P33=2 RSTA=2 RSTB=2 RSTP=2 RAMB16BWE ADDRA10=19 ADDRA11=19 ADDRA12=19 ADDRA13=19 ADDRA2=8 ADDRA3=18 ADDRA4=19 ADDRA5=19 ADDRA6=19 ADDRA7=19 ADDRA8=19 ADDRA9=19 ADDRB10=2 ADDRB11=2 ADDRB12=2 ADDRB13=2 ADDRB3=1 ADDRB4=2 ADDRB5=2 ADDRB6=2 ADDRB7=2 ADDRB8=2 ADDRB9=2 CLKA=19 CLKB=2 DIA0=6 DIA1=6 DIA10=1 DIA11=1 DIA12=1 DIA13=1 DIA14=1 DIA15=1 DIA2=6 DIA3=6 DIA4=6 DIA5=6 DIA6=6 DIA7=6 DIA8=1 DIA9=1 DIPA0=6 DIPA1=1 DOA0=17 DOA1=17 DOA2=17 DOA3=17 DOA4=9 DOA5=9 DOA6=9 DOA7=9 DOB0=2 DOB1=2 DOB10=1 DOB11=1 DOB2=2 DOB3=2 DOB4=2 DOB5=1 DOB6=1 DOB7=1 DOB8=1 DOB9=1 ENA=19 ENB=2 SSRA=19 SSRB=2 WEA0=19 WEA1=19 WEA2=19 WEA3=19 WEB0=19 WEB1=19 WEB2=19 WEB3=19 | RAMB16BWE_RAMB16BWE ADDRA10=19 ADDRA11=19 ADDRA12=19 ADDRA13=19 ADDRA2=8 ADDRA3=18 ADDRA4=19 ADDRA5=19 ADDRA6=19 ADDRA7=19 ADDRA8=19 ADDRA9=19 ADDRB10=2 ADDRB11=2 ADDRB12=2 ADDRB13=2 ADDRB3=1 ADDRB4=2 ADDRB5=2 ADDRB6=2 ADDRB7=2 ADDRB8=2 ADDRB9=2 CLKA=19 CLKB=2 DIA0=6 DIA1=6 DIA10=1 DIA11=1 DIA12=1 DIA13=1 DIA14=1 DIA15=1 DIA2=6 DIA3=6 DIA4=6 DIA5=6 DIA6=6 DIA7=6 DIA8=1 DIA9=1 DIPA0=6 DIPA1=1 DOA0=17 DOA1=17 DOA2=17 DOA3=17 DOA4=9 DOA5=9 DOA6=9 DOA7=9 DOB0=2 DOB1=2 DOB10=1 DOB11=1 DOB2=2 DOB3=2 DOB4=2 DOB5=1 DOB6=1 DOB7=1 DOB8=1 DOB9=1 ENA=19 ENB=2 SSRA=19 SSRB=2 WEA0=19 WEA1=19 WEA2=19 WEA3=19 WEB0=19 WEB1=19 WEB2=19 WEB3=19 SLICEL BX=796 BY=328 CE=1092 CIN=341 CLK=1160 COUT=351 F1=2947 F2=2760 F3=2256 F4=1633 F5=36 FX=16 FXINA=18 FXINB=18 G1=2913 G2=2734 G3=2204 G4=1489 SR=677 X=2140 XB=10 XQ=974 Y=1892 YQ=814 SLICEL_C1VDD 1=60 SLICEL_C2VDD 1=68 SLICEL_CYMUXF 0=390 1=390 OUT=390 S0=390 SLICEL_CYMUXG 0=345 1=351 OUT=351 S0=351 SLICEL_F A1=2944 A2=2760 A3=2256 A4=1633 D=2961 SLICEL_F5MUX F=507 G=507 OUT=507 S0=507 | SLICEL_F6MUX 0=18 1=18 OUT=18 S0=18 SLICEL_FFX CE=928 CK=974 D=974 Q=974 REV=2 SR=557 SLICEL_FFY CE=760 CK=814 D=814 Q=814 REV=4 SR=446 SLICEL_G A1=2910 A2=2734 A3=2204 A4=1489 D=2928 SLICEL_GNDF 0=189 SLICEL_GNDG 0=148 SLICEL_VDDG 1=6 SLICEL_XORF 0=327 1=327 O=327 SLICEL_XORG 0=310 1=310 O=310 SLICEM BX=34 BY=104 CE=40 CLK=72 F1=98 F2=98 F3=98 F4=76 F5=32 FX=16 FXINA=32 FXINB=32 G1=104 G2=104 G3=104 G4=94 SR=72 X=64 XQ=2 Y=48 YQ=40 SLICEM_F A1=98 A2=98 A3=98 A4=76 D=98 DI=66 WF1=64 WF2=64 WF3=64 WF4=64 WS=66 SLICEM_F5MUX F=32 G=32 OUT=32 S0=32 SLICEM_F6MUX 0=32 1=32 OUT=32 S0=32 SLICEM_FFX CE=2 CK=2 D=2 Q=2 SLICEM_FFY CE=40 CK=40 D=40 Q=40 SLICEM_G A1=104 A2=104 A3=104 A4=94 D=72 DI=72 WG1=64 WG2=64 WG3=64 WG4=64 WS=72 SLICEM_WSGEN CK=72 WE=72 WSF=66 WSG=72

Software Quality
Run Statistics
Bitgen | 12985 | 12984 | 0 | 0 | 0 | 0 | 0
MAP | 7079 | 6881 | 0 | 0 | 0 | 0 | 0
NGDBuild | 7397 | 7381 | 0 | 0 | 0 | 0 | 0
PAR | 6873 | 6520 | 323 | 0 | 0 | 0 | 0
Start | 0 | 0 | 0 | 0 | 0 | 0 | 0
_impact | 245 | 241 | 0 | 0 | 0 | 0 | 0
bitgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
edif2ngd | 75120 | 75116 | 0 | 0 | 0 | 0 | 0
map | 14 | 2 | 0 | 0 | 0 | 0 | 0
ngc2edif | 140 | 140 | 0 | 0 | 0 | 0 | 0
ngcbuild | 117 | 117 | 0 | 0 | 0 | 0 | 0
ngdbuild | 17 | 16 | 0 | 0 | 0 | 0 | 0
par | 2 | 2 | 0 | 0 | 0 | 0 | 0
trce | 6526 | 6522 | 0 | 0 | 0 | 0 | 0
xst | 7162 | 7059 | 0 | 0 | 0 | 0 | 0

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_AND3=1 | NGDBUILD_NUM_BUF=13 | NGDBUILD_NUM_BUFG=5 | NGDBUILD_NUM_BUFGP=2
NGDBUILD_NUM_DCM=1 | NGDBUILD_NUM_DCM_SP=1 | NGDBUILD_NUM_FD=34 | NGDBUILD_NUM_FDC=31
NGDBUILD_NUM_FDCE=685 | NGDBUILD_NUM_FDCPE=6 | NGDBUILD_NUM_FDE=794 | NGDBUILD_NUM_FDP=2
NGDBUILD_NUM_FDPE=132 | NGDBUILD_NUM_FDR=3 | NGDBUILD_NUM_FDRE=110 | NGDBUILD_NUM_FDR_1=12
NGDBUILD_NUM_FDS=11 | NGDBUILD_NUM_FDSE=11 | NGDBUILD_NUM_GND=43 | NGDBUILD_NUM_IBUF=28
NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=218 | NGDBUILD_NUM_LUT1=163 | NGDBUILD_NUM_LUT2=891
NGDBUILD_NUM_LUT2_D=44 | NGDBUILD_NUM_LUT2_L=38 | NGDBUILD_NUM_LUT3=1307 | NGDBUILD_NUM_LUT3_D=104
NGDBUILD_NUM_LUT3_L=74 | NGDBUILD_NUM_LUT4=2677 | NGDBUILD_NUM_LUT4_D=137 | NGDBUILD_NUM_LUT4_L=303
NGDBUILD_NUM_MULT18X18SIO=2 | NGDBUILD_NUM_MUXCY=720 | NGDBUILD_NUM_MUXF5=539 | NGDBUILD_NUM_MUXF6=34
NGDBUILD_NUM_MUXF7=16 | NGDBUILD_NUM_OBUF=37 | NGDBUILD_NUM_RAM16X1D=64 | NGDBUILD_NUM_RAMB16BWE=19
NGDBUILD_NUM_SRLC16E=10 | NGDBUILD_NUM_VCC=29 | NGDBUILD_NUM_XORCY=628
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_AND3=1 | NGDBUILD_NUM_BUF=13 | NGDBUILD_NUM_BUFG=7 | NGDBUILD_NUM_DCM_SP=2
NGDBUILD_NUM_FD=43 | NGDBUILD_NUM_FDC=31 | NGDBUILD_NUM_FDCE=685 | NGDBUILD_NUM_FDCPE=6
NGDBUILD_NUM_FDE=794 | NGDBUILD_NUM_FDP=2 | NGDBUILD_NUM_FDPE=132 | NGDBUILD_NUM_FDR=3
NGDBUILD_NUM_FDRE=110 | NGDBUILD_NUM_FDR_1=12 | NGDBUILD_NUM_FDS=11 | NGDBUILD_NUM_FDSE=11
NGDBUILD_NUM_GND=44 | NGDBUILD_NUM_IBUF=46 | NGDBUILD_NUM_IBUFG=3 | NGDBUILD_NUM_INV=219
NGDBUILD_NUM_LUT1=163 | NGDBUILD_NUM_LUT1_L=8 | NGDBUILD_NUM_LUT2=899 | NGDBUILD_NUM_LUT2_D=44
NGDBUILD_NUM_LUT2_L=38 | NGDBUILD_NUM_LUT3=1307 | NGDBUILD_NUM_LUT3_D=104 | NGDBUILD_NUM_LUT3_L=74
NGDBUILD_NUM_LUT4=2681 | NGDBUILD_NUM_LUT4_D=137 | NGDBUILD_NUM_LUT4_L=304 | NGDBUILD_NUM_MULT18X18SIO=2
NGDBUILD_NUM_MUXCY=721 | NGDBUILD_NUM_MUXCY_L=14 | NGDBUILD_NUM_MUXF5=539 | NGDBUILD_NUM_MUXF6=34
NGDBUILD_NUM_MUXF7=16 | NGDBUILD_NUM_OBUF=37 | NGDBUILD_NUM_RAMB16BWE=19 | NGDBUILD_NUM_SRLC16E=10
NGDBUILD_NUM_VCC=29 | NGDBUILD_NUM_XORCY=636