### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.1 (WebPack) - M.53d | Target Family: | Spartan3A and Spartan3AN
OS Platform: | NT | Target Device: | xc3s400an
Project ID (random number) | 684acf2150724198a130877b888bb684.9d76e46f0b6a4c73bf4198fb1b43096e.2 | Target Package: | fgg400
Registration ID | 176036481_0_0_631 | Target Speed: | -4
Date Generated | 2015-07-11T19:28:46 | Tool Flow | CommandLine

User Environment
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | Intel(R) Xeon(R) CPU W3520 @ 2.67GHz | CPU Speed | 2666 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
| MiscellaneousStatistics AGG_BONDED_IO=67 AGG_IO=67 AGG_SLICE=2895 NUM_4_INPUT_LUT=4814 NUM_BONDED_IBUF=5 NUM_BONDED_IOB=62 NUM_BUFGMUX=6 NUM_CYMUX=764 NUM_DCM=2 NUM_DP_RAM=256 NUM_IOB_FF=70 NUM_LUT_RT=268 NUM_MULT18X18SIO=2 NUM_MULTAND=39 NUM_RAMB16BWE=4 NUM_SLICEL=2767 NUM_SLICEM=128 NUM_SLICE_FF=2286 NUM_XOR=631 | NetStatistics NumNets_Active=5822 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BRAMADDR=80 NumNodesOfType_Active_BRAMDUMMY=208 NumNodesOfType_Active_CLKPIN=1613 NumNodesOfType_Active_CNTRLPIN=2505 NumNodesOfType_Active_DOUBLE=16068 NumNodesOfType_Active_DUMMY=14984 NumNodesOfType_Active_DUMMYBANK=72 NumNodesOfType_Active_DUMMYESC=5 NumNodesOfType_Active_GLOBAL=310 NumNodesOfType_Active_HFULLHEX=270 NumNodesOfType_Active_HLONG=75 NumNodesOfType_Active_HUNIHEX=1674 NumNodesOfType_Active_INPUT=16719 NumNodesOfType_Active_IOBOUTPUT=20 NumNodesOfType_Active_OMUX=5200 NumNodesOfType_Active_OUTPUT=5593 NumNodesOfType_Active_PREBXBY=4301 NumNodesOfType_Active_VFULLHEX=1285 NumNodesOfType_Active_VLONG=294 NumNodesOfType_Active_VUNIHEX=1943 NumNodesOfType_Gnd_BRAMADDR=8 NumNodesOfType_Gnd_BRAMDUMMY=62 NumNodesOfType_Gnd_CLKPIN=1 NumNodesOfType_Gnd_CNTRLPIN=4 NumNodesOfType_Gnd_DOUBLE=33 NumNodesOfType_Gnd_DUMMY=2 NumNodesOfType_Gnd_DUMMYBANK=5 NumNodesOfType_Gnd_HUNIHEX=1 NumNodesOfType_Gnd_INPUT=122 NumNodesOfType_Gnd_OMUX=69 NumNodesOfType_Gnd_OUTPUT=37 NumNodesOfType_Gnd_PREBXBY=48 NumNodesOfType_Gnd_VFULLHEX=3 NumNodesOfType_Gnd_VLONG=1 NumNodesOfType_Vcc_BRAMDUMMY=2 NumNodesOfType_Vcc_CLKPIN=1 NumNodesOfType_Vcc_CNTRLPIN=8 NumNodesOfType_Vcc_DUMMYBANK=3 NumNodesOfType_Vcc_INPUT=11 NumNodesOfType_Vcc_PREBXBY=6 NumNodesOfType_Vcc_VCCOUT=14 SiteStatistics IBUF-DIFFMTB=2 IBUF-DIFFSI_NDT=1 IBUF-DIFFSTB=2 IOB-DIFFMLR=24 IOB-DIFFMTB=7 IOB-DIFFSLR=25 IOB-DIFFSTB=6 SLICEL-SLICEM=1306 | SiteSummary BUFGMUX=6 BUFGMUX_GCLKMUX=6 BUFGMUX_GCLK_BUFFER=6 DCM=2 DCM_DCM=2 IBUF=5 IBUF_DELAY_ADJ_BBOX=5 IBUF_INBUF=5 IBUF_PAD=5 IOB=62 IOB_DELAY_ADJ_BBOX=16 IOB_IFF1=16 IOB_INBUF=16 IOB_OFF1=38 IOB_OUTBUF=62 IOB_PAD=62 IOB_TFF1=16 MULT18X18SIO=2 MULT18X18SIO_MULT18X18SIO=2 RAMB16BWE=4 RAMB16BWE_RAMB16BWE=4 SLICEL=2767 SLICEL_C1VDD=12 SLICEL_C2VDD=11 SLICEL_CYMUXF=390 SLICEL_CYMUXG=374 SLICEL_F=2310 SLICEL_F5MUX=275 SLICEL_F6MUX=15 SLICEL_FAND=20 SLICEL_FFX=1245 SLICEL_FFY=1041 SLICEL_G=2248 SLICEL_GAND=19 SLICEL_GNDF=233 SLICEL_GNDG=222 SLICEL_XORF=317 SLICEL_XORG=314 SLICEM=128 SLICEM_F=128 SLICEM_G=128 SLICEM_WSGEN=128

Configuration Data
BUFGMUX S=[S_INV:6] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:6] S=[S_INV:6] [S:0] DCM PSCLK=[PSCLK_INV:1] [PSCLK:1] PSEN=[PSEN_INV:1] [PSEN:1] PSINCDEC=[PSINCDEC_INV:1] [PSINCDEC:1] RST=[RST:2] [RST_INV:0] DCM_DCM CLKDV_DIVIDE=[2:1] [16:1] CLKOUT_PHASE_SHIFT=[NONE:2] CLK_FEEDBACK=[1X:2] DESKEW_ADJUST=[9:2] DFS_FREQUENCY_MODE=[LOW:2] DLL_FREQUENCY_MODE=[LOW:2] DUTY_CYCLE_CORRECTION=[TRUE:2] FACTORY_JF1=[0XC0:2] FACTORY_JF2=[0X80:2] PSCLK=[PSCLK_INV:1] [PSCLK:1] PSEN=[PSEN_INV:1] [PSEN:1] PSINCDEC=[PSINCDEC_INV:1] [PSINCDEC:1] RST=[RST:2] [RST_INV:0] IBUF_DELAY_ADJ_BBOX DELAY_ADJ_ATTRBOX=[FIXED:5] IBUF_DELAY_VALUE=[DLY0:5] IFD_DELAY_VALUE=[DLY0:5] SEL_IN=[SEL_IN:5] [SEL_IN_INV:0] IBUF_PAD IOATTRBOX=[LVTTL:5] IOB ICE=[ICE:16] [ICE_INV:0] ICLK1=[ICLK1_INV:0] [ICLK1:16] O1=[O1_INV:8] [O1:54] OCE=[OCE:0] [OCE_INV:15] OTCLK1=[OTCLK1_INV:0] [OTCLK1:38] SR=[SR:0] [SR_INV:37] T1=[T1_INV:0] [T1:16] IOB_DELAY_ADJ_BBOX DELAY_ADJ_ATTRBOX=[FIXED:16] IBUF_DELAY_VALUE=[DLY0:16] IFD_DELAY_VALUE=[DLY5:16] SEL_IN=[SEL_IN:16] [SEL_IN_INV:0] IOB_IFF1 CE=[CE:16] [CE_INV:0] CK=[CK:16] [CK_INV:0] IFF1_INIT_ATTR=[INIT0:16] IFF1_SR_ATTR=[SRLOW:16] IFFATTRBOX=[SYNC:16] LATCH_OR_FF=[FF:16] SR=[SR:0] [SR_INV:16] | IOB_OFF1 CE=[CE:0] [CE_INV:15] CK=[CK:38] [CK_INV:0] D=[D:38] [D_INV:0] LATCH_OR_FF=[FF:38] OFF1_INIT_ATTR=[INIT0:1] [INIT1:37] OFF1_SR_ATTR=[SRHIGH:37] OFFATTRBOX=[SYNC:37] SR=[SR:0] [SR_INV:37] IOB_OUTBUF IN=[IN_INV:8] [IN:54] SUSPEND=[3STATE:62] TRI=[TRI_INV:0] [TRI:16] IOB_PAD DRIVEATTRBOX=[12:62] IOATTRBOX=[LVTTL:62] SLEW=[SLOW:62] IOB_TFF1 CK=[CK:16] [CK_INV:0] D=[D:16] [D_INV:0] LATCH_OR_FF=[FF:16] SR=[SR:0] [SR_INV:16] TFF1_INIT_ATTR=[INIT1:16] TFF1_SR_ATTR=[SRHIGH:16] TFFATTRBOX=[SYNC:16] MULT18X18SIO CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] MULT18X18SIO_MULT18X18SIO AREG=[1:2] BREG=[1:2] B_INPUT=[DIRECT:2] CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] PREG=[0:2] PREG_CLKINVERSION=[0:2] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] | RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:4] CLKB=[CLKB_INV:0] [CLKB:4] ENA=[ENA_INV:0] [ENA:4] ENB=[ENB_INV:0] [ENB:4] SSRA=[SSRA_INV:0] [SSRA:4] SSRB=[SSRB_INV:0] [SSRB:4] WEA0=[WEA0:4] [WEA0_INV:0] WEA1=[WEA1:4] [WEA1_INV:0] WEA2=[WEA2:4] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:4] WEB0=[WEB0:4] [WEB0_INV:0] WEB1=[WEB1:4] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:4] WEB3=[WEB3:4] [WEB3_INV:0] RAMB16BWE_RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:4] CLKB=[CLKB_INV:0] [CLKB:4] DATA_WIDTH_A=[9:4] DATA_WIDTH_B=[9:4] ENA=[ENA_INV:0] [ENA:4] ENB=[ENB_INV:0] [ENB:4] SSRA=[SSRA_INV:0] [SSRA:4] SSRB=[SSRB_INV:0] [SSRB:4] WEA0=[WEA0:4] [WEA0_INV:0] WEA1=[WEA1:4] [WEA1_INV:0] WEA2=[WEA2:4] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:4] WEB0=[WEB0:4] [WEB0_INV:0] WEB1=[WEB1:4] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:4] WEB3=[WEB3:4] [WEB3_INV:0] WRITE_MODE_A=[WRITE_FIRST:4] WRITE_MODE_B=[WRITE_FIRST:4] SLICEL BX=[BX_INV:1] [BX:646] BY=[BY:416] [BY_INV:10] CE=[CE:1045] [CE_INV:11] CIN=[CIN_INV:0] [CIN:363] CLK=[CLK:1414] [CLK_INV:3] SR=[SR:997] [SR_INV:240] SLICEL_CYMUXF 0=[0:390] [0_INV:0] 1=[1_INV:1] [1:389] | SLICEL_CYMUXG 0=[0:374] [0_INV:0] SLICEL_F5MUX S0=[S0:275] [S0_INV:0] SLICEL_F6MUX S0=[S0:15] [S0_INV:0] SLICEL_FFX CE=[CE:944] [CE_INV:9] CK=[CK:1244] [CK_INV:1] D=[D:1245] [D_INV:0] FFX_INIT_ATTR=[INIT0:1201] [INIT1:44] FFX_SR_ATTR=[SRLOW:1208] [SRHIGH:37] LATCH_OR_FF=[FF:1245] REV=[REV_INV:0] [REV:3] SR=[SR:914] [SR_INV:176] SYNC_ATTR=[ASYNC:163] [SYNC:1082] SLICEL_FFY CE=[CE:797] [CE_INV:9] CK=[CK:1039] [CK_INV:2] D=[D:1031] [D_INV:10] FFY_INIT_ATTR=[INIT0:980] [INIT1:61] FFY_SR_ATTR=[SRLOW:984] [SRHIGH:57] LATCH_OR_FF=[FF:1041] REV=[REV_INV:0] [REV:1] SR=[SR:684] [SR_INV:199] SYNC_ATTR=[ASYNC:170] [SYNC:871] SLICEL_XORF 1=[1_INV:1] [1:316] SLICEM BY=[BY:128] [BY_INV:0] CLK=[CLK:128] [CLK_INV:0] SR=[SR:128] [SR_INV:0] SLICEM_F DI=[DI:128] [DI_INV:0] F_ATTR=[DUAL_PORT:128] LUT_OR_MEM=[RAM:128] SLICEM_G DI=[DI:128] [DI_INV:0] G_ATTR=[DUAL_PORT:128] LUT_OR_MEM=[RAM:128] SLICEM_WSGEN CK=[CK:128] [CK_INV:0] WE=[WE_INV:0] [WE:128]

Pin Data
BUFGMUX I0=6 O=6 S=6 BUFGMUX_GCLKMUX I0=6 OUT=6 S=6 BUFGMUX_GCLK_BUFFER IN=6 OUT=6 DCM CLK0=2 CLKDV=1 CLKFB=2 CLKFX=1 CLKIN=2 LOCKED=2 PSCLK=2 PSEN=2 PSINCDEC=2 RST=2 STATUS2=1 DCM_DCM CLK0=2 CLKDV=1 CLKFB=2 CLKFX=1 CLKIN=2 LOCKED=2 PSCLK=2 PSEN=2 PSINCDEC=2 RST=2 STATUS2=1 IBUF I=5 PAD=5 IBUF_DELAY_ADJ_BBOX IBUF_OUT=5 SEL_IN=5 IBUF_INBUF IN=5 OUT=5 IBUF_PAD PAD=5 IOB ICE=16 ICLK1=16 IQ1=16 O1=62 OCE=15 OTCLK1=38 PAD=62 SR=37 T1=16 IOB_DELAY_ADJ_BBOX IFD_OUT=16 SEL_IN=16 IOB_IFF1 CE=16 CK=16 D=16 Q=16 SR=16 IOB_INBUF IN=16 OUT=16 IOB_OFF1 CE=15 CK=38 D=38 Q=38 SR=37 IOB_OUTBUF IN=62 OUT=62 TRI=16 IOB_PAD PAD=62 IOB_TFF1 CK=16 D=16 Q=16 SR=16 MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=2 P16=2 P17=2 P18=2 P19=1 P2=2 P20=1 P3=2 P4=2 P5=2 P6=2 P7=2 P8=2 P9=2 RSTA=2 RSTB=2 RSTP=2 | MULT18X18SIO_MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=2 P16=2 P17=2 P18=2 P19=1 P2=2 P20=1 P3=2 P4=2 P5=2 P6=2 P7=2 P8=2 P9=2 RSTA=2 RSTB=2 RSTP=2 RAMB16BWE ADDRA10=4 ADDRA11=4 ADDRA12=4 ADDRA13=4 ADDRA3=4 ADDRA4=4 ADDRA5=4 ADDRA6=4 ADDRA7=4 ADDRA8=4 ADDRA9=4 ADDRB10=4 ADDRB11=4 ADDRB12=4 ADDRB13=4 ADDRB3=4 ADDRB4=4 ADDRB5=4 ADDRB6=4 ADDRB7=4 ADDRB8=4 ADDRB9=4 CLKA=4 CLKB=4 DIB0=4 DIB1=4 DIB2=4 DIB3=4 DIB4=4 DIB5=4 DIB6=4 DIB7=4 DIPB0=4 DOA0=4 DOA1=4 DOA2=4 DOA3=4 DOA4=4 DOA5=4 DOA6=4 DOA7=4 DOB0=4 DOB1=4 DOB2=4 DOB3=4 DOB4=4 DOB5=4 DOB6=4 DOB7=4 ENA=4 ENB=4 SSRA=4 SSRB=4 WEA0=4 WEA1=4 WEA2=4 WEA3=4 WEB0=4 WEB1=4 WEB2=4 WEB3=4 | RAMB16BWE_RAMB16BWE ADDRA10=4 ADDRA11=4 ADDRA12=4 ADDRA13=4 ADDRA3=4 ADDRA4=4 ADDRA5=4 ADDRA6=4 ADDRA7=4 ADDRA8=4 ADDRA9=4 ADDRB10=4 ADDRB11=4 ADDRB12=4 ADDRB13=4 ADDRB3=4 ADDRB4=4 ADDRB5=4 ADDRB6=4 ADDRB7=4 ADDRB8=4 ADDRB9=4 CLKA=4 CLKB=4 DIB0=4 DIB1=4 DIB2=4 DIB3=4 DIB4=4 DIB5=4 DIB6=4 DIB7=4 DIPB0=4 DOA0=4 DOA1=4 DOA2=4 DOA3=4 DOA4=4 DOA5=4 DOA6=4 DOA7=4 DOB0=4 DOB1=4 DOB2=4 DOB3=4 DOB4=4 DOB5=4 DOB6=4 DOB7=4 ENA=4 ENB=4 SSRA=4 SSRB=4 WEA0=4 WEA1=4 WEA2=4 WEA3=4 WEB0=4 WEB1=4 WEB2=4 WEB3=4 SLICEL BX=647 BY=426 CE=1056 CIN=363 CLK=1417 COUT=374 F1=2307 F2=2130 F3=1679 F4=901 F5=30 FXINA=15 FXINB=15 G1=2244 G2=2079 G3=1665 G4=905 SR=1237 X=1414 XQ=1245 Y=1385 YQ=1041 SLICEL_C1VDD 1=12 SLICEL_C2VDD 1=11 SLICEL_CYMUXF 0=390 1=390 OUT=390 S0=390 SLICEL_CYMUXG 0=374 1=374 OUT=374 S0=374 SLICEL_F A1=2299 A2=2130 A3=1679 A4=901 D=2310 SLICEL_F5MUX F=275 G=275 OUT=275 S0=275 SLICEL_F6MUX 0=15 1=15 OUT=15 S0=15 SLICEL_FAND 0=20 1=20 O=20 | SLICEL_FFX CE=953 CK=1245 D=1245 Q=1245 REV=3 SR=1090 SLICEL_FFY CE=806 CK=1041 D=1041 Q=1041 REV=1 SR=883 SLICEL_G A1=2235 A2=2077 A3=1665 A4=905 D=2248 SLICEL_GAND 0=19 1=19 O=19 SLICEL_GNDF 0=233 SLICEL_GNDG 0=222 SLICEL_XORF 0=317 1=317 O=317 SLICEL_XORG 0=314 1=314 O=314 SLICEM BY=128 CLK=128 F1=128 F2=128 F3=128 F4=128 G1=128 G2=128 G3=128 G4=128 SR=128 X=128 SLICEM_F A1=128 A2=128 A3=128 A4=128 D=128 DI=128 WF1=128 WF2=128 WF3=128 WF4=128 WS=128 SLICEM_G A1=128 A2=128 A3=128 A4=128 DI=128 WG1=128 WG2=128 WG3=128 WG4=128 WS=128 SLICEM_WSGEN CK=128 WE=128 WSF=128 WSG=128

Software Quality
Run Statistics
Bitgen | 12881 | 12880 | 0 | 0 | 0 | 0 | 0
MAP | 7026 | 6828 | 0 | 0 | 0 | 0 | 0
NGDBuild | 7343 | 7327 | 0 | 0 | 0 | 0 | 0
PAR | 6820 | 6468 | 322 | 0 | 0 | 0 | 0
Start | 0 | 0 | 0 | 0 | 0 | 0 | 0
_impact | 245 | 241 | 0 | 0 | 0 | 0 | 0
bitgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
edif2ngd | 74486 | 74482 | 0 | 0 | 0 | 0 | 0
map | 14 | 2 | 0 | 0 | 0 | 0 | 0
ngc2edif | 140 | 140 | 0 | 0 | 0 | 0 | 0
ngcbuild | 117 | 117 | 0 | 0 | 0 | 0 | 0
ngdbuild | 17 | 16 | 0 | 0 | 0 | 0 | 0
par | 2 | 2 | 0 | 0 | 0 | 0 | 0
trce | 6474 | 6470 | 0 | 0 | 0 | 0 | 0
xst | 7087 | 6984 | 0 | 0 | 0 | 0 | 0

Unisim Statistics
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_AND2=344 | NGDBUILD_NUM_AND2B1=358 | NGDBUILD_NUM_AND3=8 | NGDBUILD_NUM_AND3B1=14
NGDBUILD_NUM_AND3B2=7 | NGDBUILD_NUM_AND4B1=1 | NGDBUILD_NUM_AND4B2=1 | NGDBUILD_NUM_AND4B3=2
NGDBUILD_NUM_BUFG=6 | NGDBUILD_NUM_DCM_SP=2 | NGDBUILD_NUM_FD=25 | NGDBUILD_NUM_FDC=6
NGDBUILD_NUM_FDCE=59 | NGDBUILD_NUM_FDCPE=84 | NGDBUILD_NUM_FDE=150 | NGDBUILD_NUM_FDP=8
NGDBUILD_NUM_FDPE=4 | NGDBUILD_NUM_FDR=473 | NGDBUILD_NUM_FDRE=1505 | NGDBUILD_NUM_FDRS=1
NGDBUILD_NUM_FDRSE=3 | NGDBUILD_NUM_FDS=94 | NGDBUILD_NUM_FDSE=57 | NGDBUILD_NUM_GND=26
NGDBUILD_NUM_IBUF=21 | NGDBUILD_NUM_INV=29 | NGDBUILD_NUM_LUT1=172 | NGDBUILD_NUM_LUT1_L=147
NGDBUILD_NUM_LUT2=500 | NGDBUILD_NUM_LUT2_L=152 | NGDBUILD_NUM_LUT3=959 | NGDBUILD_NUM_LUT3_L=680
NGDBUILD_NUM_LUT4=1205 | NGDBUILD_NUM_LUT4_L=597 | NGDBUILD_NUM_MULT18X18SIO=2 | NGDBUILD_NUM_MULT_AND=39
NGDBUILD_NUM_MUXCY=87 | NGDBUILD_NUM_MUXCY_L=677 | NGDBUILD_NUM_MUXF5=284 | NGDBUILD_NUM_MUXF6=15
NGDBUILD_NUM_NAND2=6 | NGDBUILD_NUM_NOR2=3 | NGDBUILD_NUM_OBUF=46 | NGDBUILD_NUM_OBUFT=16
NGDBUILD_NUM_OR2=270 | NGDBUILD_NUM_OR2B1=7 | NGDBUILD_NUM_OR3=2 | NGDBUILD_NUM_OR3B1=3
NGDBUILD_NUM_OR3B2=3 | NGDBUILD_NUM_OR3B3=2 | NGDBUILD_NUM_OR4=11 | NGDBUILD_NUM_OR4B1=1
NGDBUILD_NUM_OR4B4=1 | NGDBUILD_NUM_RAMB16BWE=4 | NGDBUILD_NUM_VCC=17 | NGDBUILD_NUM_XNOR2=80
NGDBUILD_NUM_XORCY=629