### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.1 (WebPack) - M.53d | Target Family: | Spartan3A and Spartan3AN
OS Platform: | NT | Target Device: | xc3s400an
Project ID (random number) | 684acf2150724198a130877b888bb684.c6e1bf3459474daba571949c5e631456.2 | Target Package: | fgg400
Registration ID | 176036481_0_0_631 | Target Speed: | -4
Date Generated | 2015-07-11T19:58:47 | Tool Flow | CommandLine

User Environment
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | Intel(R) Xeon(R) CPU W3520 @ 2.67GHz | CPU Speed | 2666 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
| MiscellaneousStatistics AGG_BONDED_IO=50 AGG_IO=50 AGG_SLICE=3112 NUM_4_INPUT_LUT=5163 NUM_BONDED_IBUF=4 NUM_BONDED_IOB=46 NUM_BUFGMUX=8 NUM_CYMUX=831 NUM_DCM=3 NUM_DP_RAM=306 NUM_IOB_FF=70 NUM_LUT_RT=331 NUM_MULT18X18SIO=2 NUM_MULTAND=39 NUM_RAMB16BWE=8 NUM_SLICEL=2959 NUM_SLICEM=153 NUM_SLICE_FF=2512 NUM_XOR=770 | NetStatistics NumNets_Active=6321 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BRAMADDR=192 NumNodesOfType_Active_BRAMDUMMY=232 NumNodesOfType_Active_CLKPIN=1787 NumNodesOfType_Active_CNTRLPIN=2738 NumNodesOfType_Active_DOUBLE=17169 NumNodesOfType_Active_DUMMY=16106 NumNodesOfType_Active_DUMMYBANK=159 NumNodesOfType_Active_DUMMYESC=4 NumNodesOfType_Active_GLOBAL=280 NumNodesOfType_Active_HFULLHEX=332 NumNodesOfType_Active_HLONG=77 NumNodesOfType_Active_HUNIHEX=1827 NumNodesOfType_Active_INPUT=18066 NumNodesOfType_Active_IOBOUTPUT=20 NumNodesOfType_Active_OMUX=5599 NumNodesOfType_Active_OUTPUT=6168 NumNodesOfType_Active_PREBXBY=4631 NumNodesOfType_Active_VFULLHEX=1293 NumNodesOfType_Active_VLONG=321 NumNodesOfType_Active_VUNIHEX=1936 NumNodesOfType_Gnd_BRAMDUMMY=82 NumNodesOfType_Gnd_CLKPIN=1 NumNodesOfType_Gnd_CNTRLPIN=4 NumNodesOfType_Gnd_DOUBLE=60 NumNodesOfType_Gnd_DUMMY=127 NumNodesOfType_Gnd_DUMMYBANK=7 NumNodesOfType_Gnd_INPUT=254 NumNodesOfType_Gnd_OMUX=100 NumNodesOfType_Gnd_OUTPUT=55 NumNodesOfType_Gnd_PREBXBY=46 NumNodesOfType_Gnd_VFULLHEX=4 NumNodesOfType_Gnd_VUNIHEX=2 SiteStatistics IBUF-DIFFMTB=2 IBUF-DIFFSTB=2 IOB-DIFFMLR=20 IOB-DIFFMTB=4 IOB-DIFFSLR=19 IOB-DIFFSTB=3 SLICEL-SLICEM=1366 | SiteSummary BUFGMUX=8 BUFGMUX_GCLKMUX=8 BUFGMUX_GCLK_BUFFER=8 DCM=3 DCM_DCM=3 IBUF=4 IBUF_DELAY_ADJ_BBOX=4 IBUF_INBUF=4 IBUF_PAD=4 IOB=46 IOB_DELAY_ADJ_BBOX=16 IOB_IFF1=16 IOB_INBUF=16 IOB_OFF1=38 IOB_OUTBUF=46 IOB_PAD=46 IOB_TFF1=16 MULT18X18SIO=2 MULT18X18SIO_MULT18X18SIO=2 RAMB16BWE=8 RAMB16BWE_RAMB16BWE=8 SLICEL=2959 SLICEL_C1VDD=17 SLICEL_C2VDD=14 SLICEL_CYMUXF=424 SLICEL_CYMUXG=407 SLICEL_F=2458 SLICEL_F5MUX=260 SLICEL_F6MUX=5 SLICEL_FAND=20 SLICEL_FFX=1374 SLICEL_FFY=1113 SLICEL_G=2399 SLICEL_GAND=19 SLICEL_GNDF=265 SLICEL_GNDG=255 SLICEL_XORF=387 SLICEL_XORG=383 SLICEM=153 SLICEM_F=153 SLICEM_FFX=25 SLICEM_G=153 SLICEM_WSGEN=153

Configuration Data
BUFGMUX S=[S_INV:8] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:8] S=[S_INV:8] [S:0] DCM PSCLK=[PSCLK_INV:2] [PSCLK:1] PSEN=[PSEN_INV:2] [PSEN:1] PSINCDEC=[PSINCDEC_INV:2] [PSINCDEC:1] RST=[RST:3] [RST_INV:0] DCM_DCM CLKDV_DIVIDE=[2:2] [16:1] CLKOUT_PHASE_SHIFT=[NONE:3] CLK_FEEDBACK=[1X:3] DESKEW_ADJUST=[9:3] DFS_FREQUENCY_MODE=[LOW:3] DLL_FREQUENCY_MODE=[LOW:3] DUTY_CYCLE_CORRECTION=[TRUE:3] FACTORY_JF1=[0XC0:3] FACTORY_JF2=[0X80:3] PSCLK=[PSCLK_INV:2] [PSCLK:1] PSEN=[PSEN_INV:2] [PSEN:1] PSINCDEC=[PSINCDEC_INV:2] [PSINCDEC:1] RST=[RST:3] [RST_INV:0] IBUF_DELAY_ADJ_BBOX DELAY_ADJ_ATTRBOX=[FIXED:4] IBUF_DELAY_VALUE=[DLY0:4] IFD_DELAY_VALUE=[DLY0:4] SEL_IN=[SEL_IN:4] [SEL_IN_INV:0] IBUF_PAD IOATTRBOX=[LVCMOS25:4] IOB ICE=[ICE:16] [ICE_INV:0] ICLK1=[ICLK1_INV:0] [ICLK1:16] O1=[O1_INV:0] [O1:46] OCE=[OCE:0] [OCE_INV:15] OTCLK1=[OTCLK1_INV:0] [OTCLK1:38] SR=[SR:37] [SR_INV:0] T1=[T1_INV:0] [T1:16] IOB_DELAY_ADJ_BBOX DELAY_ADJ_ATTRBOX=[FIXED:16] IBUF_DELAY_VALUE=[DLY0:16] IFD_DELAY_VALUE=[DLY5:16] SEL_IN=[SEL_IN:16] [SEL_IN_INV:0] IOB_IFF1 CE=[CE:16] [CE_INV:0] CK=[CK:16] [CK_INV:0] IFF1_INIT_ATTR=[INIT0:16] IFF1_SR_ATTR=[SRLOW:16] IFFATTRBOX=[SYNC:16] LATCH_OR_FF=[FF:16] SR=[SR:16] [SR_INV:0] | IOB_OFF1 CE=[CE:0] [CE_INV:15] CK=[CK:38] [CK_INV:0] D=[D:38] [D_INV:0] LATCH_OR_FF=[FF:38] OFF1_INIT_ATTR=[INIT0:1] [INIT1:37] OFF1_SR_ATTR=[SRHIGH:37] OFFATTRBOX=[SYNC:37] SR=[SR:37] [SR_INV:0] IOB_OUTBUF IN=[IN_INV:0] [IN:46] SUSPEND=[3STATE:46] TRI=[TRI_INV:0] [TRI:16] IOB_PAD DRIVEATTRBOX=[12:46] IOATTRBOX=[LVCMOS25:46] SLEW=[SLOW:46] IOB_TFF1 CK=[CK:16] [CK_INV:0] D=[D:16] [D_INV:0] LATCH_OR_FF=[FF:16] SR=[SR:16] [SR_INV:0] TFF1_INIT_ATTR=[INIT1:16] TFF1_SR_ATTR=[SRHIGH:16] TFFATTRBOX=[SYNC:16] MULT18X18SIO CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] MULT18X18SIO_MULT18X18SIO AREG=[1:2] BREG=[1:2] B_INPUT=[DIRECT:2] CEA=[CEA_INV:0] [CEA:2] CEB=[CEB_INV:0] [CEB:2] CEP=[CEP:2] [CEP_INV:0] CLK=[CLK:2] [CLK_INV:0] PREG=[0:2] PREG_CLKINVERSION=[0:2] RSTA=[RSTA:2] [RSTA_INV:0] RSTB=[RSTB:2] [RSTB_INV:0] RSTP=[RSTP_INV:0] [RSTP:2] | RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:8] CLKB=[CLKB_INV:0] [CLKB:8] ENA=[ENA_INV:0] [ENA:8] ENB=[ENB_INV:0] [ENB:8] SSRA=[SSRA_INV:0] [SSRA:8] SSRB=[SSRB_INV:0] [SSRB:8] WEA0=[WEA0:8] [WEA0_INV:0] WEA1=[WEA1:8] [WEA1_INV:0] WEA2=[WEA2:8] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:8] WEB0=[WEB0:8] [WEB0_INV:0] WEB1=[WEB1:8] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:8] WEB3=[WEB3:8] [WEB3_INV:0] RAMB16BWE_RAMB16BWE CLKA=[CLKA_INV:0] [CLKA:8] CLKB=[CLKB_INV:0] [CLKB:8] DATA_WIDTH_A=[4:8] DATA_WIDTH_B=[4:8] ENA=[ENA_INV:0] [ENA:8] ENB=[ENB_INV:0] [ENB:8] SSRA=[SSRA_INV:0] [SSRA:8] SSRB=[SSRB_INV:0] [SSRB:8] WEA0=[WEA0:8] [WEA0_INV:0] WEA1=[WEA1:8] [WEA1_INV:0] WEA2=[WEA2:8] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:8] WEB0=[WEB0:8] [WEB0_INV:0] WEB1=[WEB1:8] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:8] WEB3=[WEB3:8] [WEB3_INV:0] WRITE_MODE_A=[WRITE_FIRST:8] WRITE_MODE_B=[WRITE_FIRST:8] SLICEL BX=[BX_INV:1] [BX:660] BY=[BY:465] [BY_INV:9] CE=[CE:1083] [CE_INV:14] CIN=[CIN_INV:0] [CIN:404] CLK=[CLK:1553] [CLK_INV:3] SR=[SR:1376] [SR_INV:27] SLICEL_CYMUXF 0=[0:424] [0_INV:0] 1=[1_INV:1] [1:423] | SLICEL_CYMUXG 0=[0:407] [0_INV:0] SLICEL_F5MUX S0=[S0:260] [S0_INV:0] SLICEL_F6MUX S0=[S0:5] [S0_INV:0] SLICEL_FFX CE=[CE:977] [CE_INV:11] CK=[CK:1373] [CK_INV:1] D=[D:1374] [D_INV:0] FFX_INIT_ATTR=[INIT0:1329] [INIT1:45] FFX_SR_ATTR=[SRLOW:1335] [SRHIGH:39] LATCH_OR_FF=[FF:1374] REV=[REV_INV:0] [REV:3] SR=[SR:1219] [SR_INV:16] SYNC_ATTR=[ASYNC:295] [SYNC:1079] SLICEL_FFY CE=[CE:832] [CE_INV:12] CK=[CK:1110] [CK_INV:3] D=[D:1104] [D_INV:9] FFY_INIT_ATTR=[INIT0:1050] [INIT1:63] FFY_SR_ATTR=[SRLOW:1054] [SRHIGH:59] LATCH_OR_FF=[FF:1113] REV=[REV_INV:0] [REV:1] SR=[SR:975] [SR_INV:20] SYNC_ATTR=[ASYNC:249] [SYNC:864] SLICEL_XORF 1=[1_INV:1] [1:386] SLICEM BY=[BY:153] [BY_INV:0] CLK=[CLK:153] [CLK_INV:0] SR=[SR:153] [SR_INV:0] SLICEM_F DI=[DI:153] [DI_INV:0] F_ATTR=[DUAL_PORT:153] LUT_OR_MEM=[RAM:153] SLICEM_FFX CK=[CK:25] [CK_INV:0] D=[D:25] [D_INV:0] FFX_INIT_ATTR=[INIT0:25] FFX_SR_ATTR=[SRLOW:25] LATCH_OR_FF=[FF:25] SYNC_ATTR=[ASYNC:25] SLICEM_G DI=[DI:153] [DI_INV:0] G_ATTR=[DUAL_PORT:153] LUT_OR_MEM=[RAM:153] SLICEM_WSGEN CK=[CK:153] [CK_INV:0] SYNC_ATTR=[ASYNC:25] WE=[WE_INV:0] [WE:153] |

Pin Data
BUFGMUX I0=8 O=8 S=8 BUFGMUX_GCLKMUX I0=8 OUT=8 S=8 BUFGMUX_GCLK_BUFFER IN=8 OUT=8 DCM CLK0=3 CLKDV=1 CLKFB=3 CLKFX=2 CLKIN=3 LOCKED=3 PSCLK=3 PSEN=3 PSINCDEC=3 RST=3 STATUS2=2 DCM_DCM CLK0=3 CLKDV=1 CLKFB=3 CLKFX=2 CLKIN=3 LOCKED=3 PSCLK=3 PSEN=3 PSINCDEC=3 RST=3 STATUS2=2 IBUF I=4 PAD=4 IBUF_DELAY_ADJ_BBOX IBUF_OUT=4 SEL_IN=4 IBUF_INBUF IN=4 OUT=4 IBUF_PAD PAD=4 IOB ICE=16 ICLK1=16 IQ1=16 O1=46 OCE=15 OTCLK1=38 PAD=46 SR=37 T1=16 IOB_DELAY_ADJ_BBOX IFD_OUT=16 SEL_IN=16 IOB_IFF1 CE=16 CK=16 D=16 Q=16 SR=16 IOB_INBUF IN=16 OUT=16 IOB_OFF1 CE=15 CK=38 D=38 Q=38 SR=37 IOB_OUTBUF IN=46 OUT=46 TRI=16 IOB_PAD PAD=46 IOB_TFF1 CK=16 D=16 Q=16 SR=16 MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=2 P16=2 P17=2 P18=2 P19=1 P2=2 P20=1 P3=2 P4=2 P5=2 P6=2 P7=2 P8=2 P9=2 RSTA=2 RSTB=2 RSTP=2 | MULT18X18SIO_MULT18X18SIO A0=2 A1=2 A10=2 A11=2 A12=2 A13=2 A14=2 A15=2 A16=2 A17=2 A2=2 A3=2 A4=2 A5=2 A6=2 A7=2 A8=2 A9=2 B0=2 B1=2 B10=2 B11=2 B12=2 B13=2 B14=2 B15=2 B16=2 B17=2 B2=2 B3=2 B4=2 B5=2 B6=2 B7=2 B8=2 B9=2 CEA=2 CEB=2 CEP=2 CLK=2 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=2 P16=2 P17=2 P18=2 P19=1 P2=2 P20=1 P3=2 P4=2 P5=2 P6=2 P7=2 P8=2 P9=2 RSTA=2 RSTB=2 RSTP=2 RAMB16BWE ADDRA10=8 ADDRA11=8 ADDRA12=8 ADDRA13=8 ADDRA2=8 ADDRA3=8 ADDRA4=8 ADDRA5=8 ADDRA6=8 ADDRA7=8 ADDRA8=8 ADDRA9=8 ADDRB10=8 ADDRB11=8 ADDRB12=8 ADDRB13=8 ADDRB2=8 ADDRB3=8 ADDRB4=8 ADDRB5=8 ADDRB6=8 ADDRB7=8 ADDRB8=8 ADDRB9=8 CLKA=8 CLKB=8 DIB0=8 DIB1=8 DIB2=8 DIB3=8 DOA0=8 DOA1=8 DOA2=8 DOA3=8 DOB0=8 DOB1=8 DOB2=8 DOB3=8 ENA=8 ENB=8 SSRA=8 SSRB=8 WEA0=8 WEA1=8 WEA2=8 WEA3=8 WEB0=8 WEB1=8 WEB2=8 WEB3=8 | RAMB16BWE_RAMB16BWE ADDRA10=8 ADDRA11=8 ADDRA12=8 ADDRA13=8 ADDRA2=8 ADDRA3=8 ADDRA4=8 ADDRA5=8 ADDRA6=8 ADDRA7=8 ADDRA8=8 ADDRA9=8 ADDRB10=8 ADDRB11=8 ADDRB12=8 ADDRB13=8 ADDRB2=8 ADDRB3=8 ADDRB4=8 ADDRB5=8 ADDRB6=8 ADDRB7=8 ADDRB8=8 ADDRB9=8 CLKA=8 CLKB=8 DIB0=8 DIB1=8 DIB2=8 DIB3=8 DOA0=8 DOA1=8 DOA2=8 DOA3=8 DOB0=8 DOB1=8 DOB2=8 DOB3=8 ENA=8 ENB=8 SSRA=8 SSRB=8 WEA0=8 WEA1=8 WEA2=8 WEA3=8 WEB0=8 WEB1=8 WEB2=8 WEB3=8 SLICEL BX=661 BY=474 CE=1097 CIN=404 CLK=1556 COUT=407 F1=2458 F2=2239 F3=1843 F4=996 F5=10 FXINA=5 FXINB=5 G1=2399 G2=2191 G3=1804 G4=1021 SR=1403 X=1503 XQ=1374 Y=1545 YQ=1113 SLICEL_C1VDD 1=17 SLICEL_C2VDD 1=14 SLICEL_CYMUXF 0=424 1=424 OUT=424 S0=424 SLICEL_CYMUXG 0=407 1=407 OUT=407 S0=407 SLICEL_F A1=2450 A2=2239 A3=1843 A4=996 D=2458 SLICEL_F5MUX F=260 G=260 OUT=260 S0=260 SLICEL_F6MUX 0=5 1=5 OUT=5 S0=5 SLICEL_FAND 0=20 1=20 O=20 SLICEL_FFX CE=988 CK=1374 D=1374 Q=1374 REV=3 SR=1235 | SLICEL_FFY CE=844 CK=1113 D=1113 Q=1113 REV=1 SR=995 SLICEL_G A1=2390 A2=2189 A3=1804 A4=1021 D=2399 SLICEL_GAND 0=19 1=19 O=19 SLICEL_GNDF 0=265 SLICEL_GNDG 0=255 SLICEL_XORF 0=387 1=387 O=387 SLICEL_XORG 0=383 1=383 O=383 SLICEM BY=153 CLK=153 F1=153 F2=153 F3=153 F4=153 G1=153 G2=153 G3=153 G4=153 SR=153 X=128 XQ=25 Y=23 SLICEM_F A1=153 A2=153 A3=153 A4=153 D=153 DI=153 WF1=153 WF2=153 WF3=153 WF4=153 WS=153 SLICEM_FFX CK=25 D=25 Q=25 SLICEM_G A1=153 A2=153 A3=153 A4=153 D=23 DI=153 WG1=153 WG2=153 WG3=153 WG4=153 WS=153 SLICEM_WSGEN CK=153 WE=153 WSF=153 WSG=153

Software Quality
Run Statistics
Bitgen | 12887 | 12886 | 0 | 0 | 0 | 0 | 0
MAP | 7029 | 6831 | 0 | 0 | 0 | 0 | 0
NGDBuild | 7346 | 7330 | 0 | 0 | 0 | 0 | 0
PAR | 6823 | 6471 | 322 | 0 | 0 | 0 | 0
Start | 0 | 0 | 0 | 0 | 0 | 0 | 0
_impact | 245 | 241 | 0 | 0 | 0 | 0 | 0
bitgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
edif2ngd | 74510 | 74506 | 0 | 0 | 0 | 0 | 0
map | 14 | 2 | 0 | 0 | 0 | 0 | 0
ngc2edif | 140 | 140 | 0 | 0 | 0 | 0 | 0
ngcbuild | 117 | 117 | 0 | 0 | 0 | 0 | 0
ngdbuild | 17 | 16 | 0 | 0 | 0 | 0 | 0
par | 2 | 2 | 0 | 0 | 0 | 0 | 0
trce | 6477 | 6473 | 0 | 0 | 0 | 0 | 0
xst | 7089 | 6986 | 0 | 0 | 0 | 0 | 0

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUF=5 | NGDBUILD_NUM_BUFG=4 | NGDBUILD_NUM_DCM_SP=1 | NGDBUILD_NUM_FD=49
NGDBUILD_NUM_FDC=111 | NGDBUILD_NUM_FDCE=156 | NGDBUILD_NUM_FDE=8 | NGDBUILD_NUM_FDP=1
NGDBUILD_NUM_FDR=75 | NGDBUILD_NUM_FDRE=32 | NGDBUILD_NUM_GND=13 | NGDBUILD_NUM_IBUF=3
NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=20 | NGDBUILD_NUM_IOBUF=16 | NGDBUILD_NUM_LUT1=35
NGDBUILD_NUM_LUT2=184 | NGDBUILD_NUM_LUT2_L=2 | NGDBUILD_NUM_LUT3=106 | NGDBUILD_NUM_LUT3_L=1
NGDBUILD_NUM_LUT4=219 | NGDBUILD_NUM_LUT4_D=2 | NGDBUILD_NUM_LUT4_L=21 | NGDBUILD_NUM_MUXCY=120
NGDBUILD_NUM_MUXF5=2 | NGDBUILD_NUM_NAND3=1 | NGDBUILD_NUM_OBUF=30 | NGDBUILD_NUM_RAM16X1D=25
NGDBUILD_NUM_VCC=8 | NGDBUILD_NUM_XORCY=124
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_AND2=8 | NGDBUILD_NUM_BUF=5 | NGDBUILD_NUM_BUFG=8 | NGDBUILD_NUM_DCM_SP=3
NGDBUILD_NUM_FD=62 | NGDBUILD_NUM_FDC=114 | NGDBUILD_NUM_FDCE=211 | NGDBUILD_NUM_FDCPE=1
NGDBUILD_NUM_FDC_1=4 | NGDBUILD_NUM_FDE=168 | NGDBUILD_NUM_FDP=9 | NGDBUILD_NUM_FDPE=3
NGDBUILD_NUM_FDR=475 | NGDBUILD_NUM_FDRE=1490 | NGDBUILD_NUM_FDRS=1 | NGDBUILD_NUM_FDRSE=3
NGDBUILD_NUM_FDS=95 | NGDBUILD_NUM_FDSE=59 | NGDBUILD_NUM_GND=34 | NGDBUILD_NUM_IBUF=19
NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=37 | NGDBUILD_NUM_LUT1=207 | NGDBUILD_NUM_LUT1_L=177
NGDBUILD_NUM_LUT2=699 | NGDBUILD_NUM_LUT2_L=197 | NGDBUILD_NUM_LUT3=1081 | NGDBUILD_NUM_LUT3_L=744
NGDBUILD_NUM_LUT4=1470 | NGDBUILD_NUM_LUT4_D=2 | NGDBUILD_NUM_LUT4_L=625 | NGDBUILD_NUM_MULT18X18SIO=2
NGDBUILD_NUM_MULT_AND=39 | NGDBUILD_NUM_MUXCY=124 | NGDBUILD_NUM_MUXCY_L=707 | NGDBUILD_NUM_MUXF5=269
NGDBUILD_NUM_MUXF6=5 | NGDBUILD_NUM_NAND3=1 | NGDBUILD_NUM_OBUF=30 | NGDBUILD_NUM_OBUFT=16
NGDBUILD_NUM_RAMB16BWE=8 | NGDBUILD_NUM_VCC=20 | NGDBUILD_NUM_XORCY=770